
Format(s): 
B-Format (4 Channel Files)

B-Format: Multichannel: 

    kick_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Kick Drum position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.46 m
Source Height: 0.25 m
Receiver Height: 1.70 m
Temperature: 21 °C


    snare_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Snare Drum Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.46 m
Source Height: 0.67 m
Receiver Height: 1.70 m
Temperature: 21 °C


    toma_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Tom A Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.21 m
Source Height: 0.87 m
Receiver Height: 1.70 m
Temperature: 21 °C


    tomb_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Tom B Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.23 m
Source Height: 0.87 m
Receiver Height: 1.70 m
Temperature: 21 °C


    tomc_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Floor Tom Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.41 m
Source Height: 0.77 m
Receiver Height: 1.70 m
Temperature: 21 °C


    hh_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Hi Hat Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.43 m
Source Height: 1.04 m
Receiver Height: 1.70 m
Temperature: 21 °C


    crash_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Crash Cymbal Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.13 m
Source Height: 1.17 m
Receiver Height: 1.70 m
Temperature: 21 °C


    ride_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 2 s
File Size: 2.2 MB
File Format: wav
Source Sound: 10 Second Exponential Sine Sweep (20Hz - 20kHz)
Microphone: Soundfield ST350 Kit
Source Location: Ride Cymbal Position
Microphone Location: Opposite the source 76cm from wall
Source Receiver Distance (m): 2.17 m
Source Height: 1.17 m
Receiver Height: 1.70 m
Temperature: 21 °C

