
Format(s): 
B-Format (4 Channel Files)

B-Format: Multichannel: 

    ir_p1.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, 3.82m left of curve. (See schematic image 1)
Microphone Location: Centre of pathway, center of curve. (See schematic image 1)
Source Receiver Distance (m): 3.82 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C


    ir_p2.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, 3.82m left to center of curve. (See schematic image 1)
Microphone Location: Centre of pathway, right of curve. (See schematic image 1)
Source Receiver Distance (m): 6 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C


    ir_p3.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, 3.82m left of curve. (See schematic image 1).
Microphone Location: Left of pathway, right of curve. (See schematic image 1). IR a little corrupted by the presence of water drips.
Source Receiver Distance (m): 11.1 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C


    ir_p4.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, 3.82m left of curve. (See schematic image 1)
Microphone Location: Right of pathway, right of curve. (See schematic image 1). IR a little corrupted by the presence of water drips.
Source Receiver Distance (m): 13.7 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C


    ir_p5.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, just right of curve. (See schematic image 2)
Microphone Location: Centre of pathway, right of curve. (See schematic image 2)
Source Receiver Distance (m): 3 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C


    ir_p6.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 16
Duration: 2 s
File Size: 1.46 MB
File Format: wav
Source Sound: Genelec 8130A
Microphone: Soundfield ST450 MKII Microphone
Source Location: Centre of pathway, just right of curve. (See schematic image 2).
Microphone Location: Centre of pathway, right of curve, next to opening. (See schematic image 2). IR a little corrupted by the presence of water drips.
Source Receiver Distance (m): 6 m
Source Height: 1.5 m
Receiver Height: 1.2 m
Temperature: 5 °C