
Format(s): 
Mono
Stereo (Stereo Files)
5.1 Surround (6 Channel Files)
B-Format (4 Channel Files)

Mono: 

    r1_omni.wav

Sample Rate: 44.1 kHz
Number of Channels: 1
Bits per Sample: 24
Duration: 19.94 s
File Size: 2.52 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m


    r1_omni_48k.wav

Sample Rate: 48 kHz
Number of Channels: 1
Bits per Sample: 24
Duration: 19.94 s
File Size: 2.74 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m

Stereo: 

    r1_ortf.wav

Sample Rate: 44.1 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 20.28 s
File Size: 5.12 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Cardioid Microphone, Neumann KM 140
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m


    r1_ortf-48k.wav

Sample Rate: 48 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 20.28 s
File Size: 5.57 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Cardioid Microphone, Neumann KM 140
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m

B-Format: Multichannel: 

    r1_bformat.wav

Sample Rate: 44.1 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 14.8 s
File Size: 7.47 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m


    r1_bformat-48k.wav

Sample Rate: 48 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 8.8 s
File Size: 4.83 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m

5.1 Surround: 

    r1_williams.wav

Sample Rate: 44.1 kHz
Number of Channels: 6
Bits per Sample: 24
Duration: 9.8 s
File Size: 7.42 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m


    r1_williams-48k.wav

Sample Rate: 48 kHz
Number of Channels: 6
Bits per Sample: 24
Duration: 8.8 s
File Size: 7.25 MB
File Format: wav
Source Sound: Genelec 8240A loudspeaker, 15 second log. sine sweep
Microphone: Soundfield Microphone, SPS422B
Source Location: In the centre, on one side of the pit
Microphone Location: In the centre, on other side of the pit
Source Receiver Distance (m): 14.88 m
Source Height: 1.5 m
Receiver Height: 1.5 m