
Format(s): 
B-Format (4 Channel Files)

B-Format: Multichannel: 

    fsfr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Source Location: First Source
Microphone Location: First Receiver
Source Receiver Distance (m): 12.6 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    fssr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Source Location: First Source
Microphone Location: Second Receiver
Source Receiver Distance (m): 19.3 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    fstr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: First Source
Microphone Location: Third Receiver Position
Source Receiver Distance (m): 34.7 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    ssfr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Second Source
Microphone Location: First Receiver
Source Receiver Distance (m): 13.8 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    sssr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Second Source
Microphone Location: Second Receiver
Source Receiver Distance (m): 15.9 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    sstr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Second Source
Microphone Location: Third Receiver
Source Receiver Distance (m): 18 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    tsfr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Third Source
Microphone Location: First Receiver
Source Receiver Distance (m): 33 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    tsfthr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Third Source
Microphone Location: Fourth Receiver
Source Receiver Distance (m): 11 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    tssr.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Third Source
Microphone Location: Second Receiver
Source Receiver Distance (m): 32 m
Source Height: 1.5 m
Receiver Height: 1.2 m


    tstr_ir.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 1.1 MB
File Format: wav
Source Sound: Exponential Sine Sweep
Microphone: ST450
Source Location: Third Source
Microphone Location: Third Receiver
Source Receiver Distance (m): 4.5 m
Source Height: 1.5 m
Receiver Height: 1.2 m

