
Format(s): 
B-Format (4 Channel Files)

B-Format: Multichannel: 

    councilchamber_s1_r1_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 1 - Mayor's Chair
Microphone Location: Receiver Position 1 - Public Pews Centre
Source Receiver Distance (m): 12 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s1_r2_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 1 - Mayor's Chair
Microphone Location: Receiver Position 2 - Counsellor Seating (NW Side)
Source Receiver Distance (m): 9.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s1_r3_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 1 - Mayor's Chair
Microphone Location: Receiver Position 3 - Counsellor Seating (NE Side)
Source Receiver Distance (m): 9.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s1_r4_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 1 - Mayor's Chair
Microphone Location: Receiver Position 4 - Counsellor Seating (Central)
Source Receiver Distance (m): 7.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s2_r1_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 2 - Counsellor Seating (North Side)
Microphone Location: Receiver Position 1 - Public Pews Centre
Source Receiver Distance (m): 6.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s2_r2_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 2 - Counsellor Seating (North Side)
Microphone Location: Receiver Position 2 - Counsellor Seating (NW Side)
Source Receiver Distance (m): 4.50 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s2_r3_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 2 - Counsellor Seating (North Side)
Microphone Location: Receiver Position 3 - Counsellor Seating (NE Side)
Source Receiver Distance (m): 3.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s2_r4_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 2 - Counsellor Seating (North Side)
Microphone Location: Receiver Position 4 - Counsellor Seating (Central)
Source Receiver Distance (m): 3.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s3_r1_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 3 - Counsellor Seating (South Side)
Microphone Location: Receiver Position 1 - Public Pews Centre
Source Receiver Distance (m): 6.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s3_r2_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 3 - Counsellor Seating (South Side)
Microphone Location: Receiver Position 2 - Counsellor Seating (NW Side)
Source Receiver Distance (m): 3.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s3_r3_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 3 - Counsellor Seating (South Side)
Microphone Location: Receiver Position 3 - Counsellor Seating (NE Side)
Source Receiver Distance (m): 4.50 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C


    councilchamber_s3_r4_ir_1_96000.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 5 s
File Size: 5.49 MB
File Format: wav
Source Sound: Genelec 8130A. 30 Second Logarithmic Sine Sweep, 20 Hz - 22 kHz.
Microphone: Soundfield ST450 MkII
Source Location: Source Position 3 - Counsellor Seating (South Side)
Microphone Location: Receiver Position 4 - Counsellor Seating (Central)
Source Receiver Distance (m): 3.0 m
Source Height: 1.60 m
Receiver Height: 1.60 m
Temperature: 16 °C