
Format(s): 
B-Format (4 Channel Files)

B-Format: Multichannel: 

    s1r2.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Center of the stage
Microphone Location: Center seat, middle row
Source Receiver Distance (m): 7.6 m
Source Height: 1.5 m
Receiver Height: 3 m
Temperature: 20 °C


    s1r4.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Center of the stage
Microphone Location: Center, top row
Source Receiver Distance (m): 12.9 m
Source Height: 1.5 m
Receiver Height: 4.5 m
Temperature: 20 °C


    s1r7.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Center of the stage
Microphone Location: Balcony, above and behind the source.
Source Receiver Distance (m): 3.3 m
Source Height: 1.5 m
Receiver Height: 4.5 m
Temperature: 20 °C


    s2r4.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Right corner of the stage, pointing towards the sweetspot on the center seat of the middle row.
Microphone Location: Center, top row
Source Receiver Distance (m): 13.5 m
Source Height: 1.5 m
Receiver Height: 4.5 m
Temperature: 20 °C


    s2r6.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Right corner of the stage, pointing towards the sweetspot on the center seat of the middle row.
Microphone Location: Right side up in the balcony.
Source Receiver Distance (m): 9.5 m
Source Height: 1.5 m
Receiver Height: 3 m
Temperature: 20 °C


    s2r7.wav

Sample Rate: 96 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1.5 s
File Size: 1.65 MB
File Format: wav
Source Sound: Genelec 8030, ESS 25 seconds, 20 Hz to 20 kHz
Microphone: Soundfield ST350 Kit
Source Location: Right corner of the stage, pointing towards the sweetspot on the center seat of the middle row.
Microphone Location: Above and behind the source. Up in the balcony.
Source Receiver Distance (m): 4.1 m
Source Height: 1.5 m
Receiver Height: 4.5 m
Temperature: 20 °C