
Format(s): 
Mono
Stereo (Stereo Files)
5.1 Surround (6 Channel Files)
B-Format (4 Channel Files)

Mono: 

    stalbans_a_mono.wav

Sample Rate: 44.1 kHz
Number of Channels: 1
Bits per Sample: 24
Duration: 6 s
File Size: 775.3 KB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Neumann KM 140 Cardioid
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_b_mono.wav

Sample Rate: 44.1 kHz
Number of Channels: 1
Bits per Sample: 24
Duration: 6 s
File Size: 775.3 KB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Neumann KM 140 Cardioid
Source Location: B
Microphone Location: B
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_omni.wav

Sample Rate: 44.1 kHz
Number of Channels: 1
Bits per Sample: 24
Duration: 6 s
File Size: 775.3 KB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Soundfield SPS422B Microphone
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m

Stereo: 

    stalbans_a_ortf.wav

Sample Rate: 44.1 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 6 s
File Size: 1.51 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Neumann KM 140 Cardioid
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_b_ortf.wav

Sample Rate: 44.1 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 6 s
File Size: 1.51 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Neumann KM 140 Cardioid
Source Location: B
Microphone Location: B
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_a_binaural.wav

Sample Rate: 44.1 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 6 s
File Size: 1.51 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_b_binaural.wav

Sample Rate: 44.1 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 6 s
File Size: 1.51 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Source Location: B
Microphone Location: B
Source Height: 1.5 m
Receiver Height: 1.5 m

B-Format: Multichannel: 

    stalbans_a_wxyz.wav

Sample Rate: 44.1 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 6 s
File Size: 3.03 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Soundfield SPS422B Microphone
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_b_wxyz.wav

Sample Rate: 44.1 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 6 s
File Size: 3.03 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Soundfield SPS422B Microphone
Source Location: B
Microphone Location: B
Source Height: 1.5 m
Receiver Height: 1.5 m

5.1 Surround: 

    stalbans_a_williams.wav

Sample Rate: 44.1 kHz
Number of Channels: 6
Bits per Sample: 24
Duration: 6 s
File Size: 4.54 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Soundfield SPS422B Microphone
Source Location: A
Microphone Location: A
Source Height: 1.5 m
Receiver Height: 1.5 m


    stalbans_b_williams.wav

Sample Rate: 44.1 kHz
Number of Channels: 6
Bits per Sample: 24
Duration: 6 s
File Size: 4.54 MB
File Format: wav
Source Sound: Genelec S30D, 10 second log. sine sweep
Microphone: Soundfield SPS422B Microphone
Source Location: B
Microphone Location: B
Source Height: 1.5 m
Receiver Height: 1.5 m

