
Format(s): 
Stereo (Stereo Files)
B-Format (4 Channel Files)

Stereo: 

    mh3_000_ortf_48k.wav

Sample Rate: 48 kHz
Number of Channels: 2
Bits per Sample: 24
Duration: 1 s
File Size: 281.29 KB
File Format: wav
Source Sound: Genelec S30D, 15 second log. sine sweep
Microphone: Neumann KM 140 Cardioid
Source Location: Centre of chamber
Microphone Location: Centre of wall opposite entrance
Source Receiver Distance (m): 2 m
Source Height: 1.5 m
Receiver Height: 1.5 m
Temperature: 10 °C

B-Format: Multichannel: 

    mh3_000_bformat_48k.wav

Sample Rate: 48 kHz
Number of Channels: 4
Bits per Sample: 24
Duration: 1 s
File Size: 562.62 KB
File Format: wav
Source Sound: Genelec S30D, 15 second log. sine sweep
Microphone: Soundfield SPS422B
Source Location: Centre of chamber
Microphone Location: Centre of wall opposite entrance
Source Receiver Distance (m): 2 m
Source Height: 1.5 m
Receiver Height: 1.5 m
Temperature: 10 °C